

|  |  |
| --- | --- |
|  | Addressable I/O Module AW-D319Data Sheet  |
| Operating Voltage  | Signal Loop 24V(18V～28V) Power 24VDC(20VDC～28VDC)  |
| Standby Current  | Loop＜0.8mA ; Power＜2mA  |
| Action Current  | Loop＜5mA ; Power＜15mA  |
| Output Capacity  | 1A@DC30V |
| Input Mode Setting | NC or NO input mode can be set by the jumper JP4. |
| Programming Method  | Electronically addressed  |
| Code Range  | One address within 1~324.  |
| Indicators  | Inspection indicator: l blink once about every 12 seconds in the inspection status or remain lit in the output status; Input indicator : remain lit in the feedback status. |
| Operating Temperature  | -10℃～+55℃  |
| Relative Humidity  | ≤95% , non-condensing  |
| Material of Enclosure  | ABS  |
| Dimension (L×W×H)  | 86mm×86mm×41mm (with base)  |
| Mounting Hole Distance  | 60.5mm |
| Weight  | About 148g (with base)  |
| Certificate |  |