

|  |  |
| --- | --- |
|  | Addressable I/O Module  AW-D319  Data Sheet |
| Operating Voltage | Signal Loop 24V(18V～28V)  Power 24VDC(20VDC～28VDC) |
| Standby Current | Loop＜0.8mA ; Power＜2mA |
| Action Current | Loop＜5mA ; Power＜15mA |
| Output Capacity | 1A@DC30V |
| Input Mode Setting | NC or NO input mode can be set by the jumper JP4. |
| Programming Method | Electronically addressed |
| Code Range | One address within 1~324. |
| Indicators | Inspection indicator: l blink once about every 12 seconds in the inspection status or remain lit in the output status;  Input indicator : remain lit in the feedback status. |
| Operating Temperature | -10℃～+55℃ |
| Relative Humidity | ≤95% , non-condensing |
| Material of Enclosure | ABS |
| Dimension (L×W×H) | 86mm×86mm×41mm  (with base) |
| Mounting Hole Distance | 60.5mm |
| Weight | About 148g (with base) |
| Certificate |  |